[16] ENGINE ELECTRICAL - - CHARGING SYSTEM - ALTERNATOR ASSEMBLY - REMOVAL AND INSTALLATION <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G69>
Pre-removal Operation Under Cover Removal (Refer to GROUP 51, Under Cover ). Drive Belt Removal (Refer to GROUP 11E, Crankshaft Pulley ). | Post-installation Operation Drive Belt Installation (Refer to GROUP 11E, Crankshaft Pulley ). Drive Belt Tension Check (Refer to GROUP 11E, On-vehicle Service ). Under Cover Installation (Refer to GROUP 51, Under Cover ).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | A/C compressor assembly connector
|  | 2. | A/C compressor assembly connector clamp
|  | 3. | Alternator connector
|  | 4. | Alternator terminal
|  | 5. | Connector bracket
|  | 6. | Harness bracket
<<A>> |  | 7. | Alternator assembly
|  | • | Timing belt lower cover (Refer to GROUP 11E, Timing Belt ).
|  | 8. | Alternator mounting bracket
| REMOVAL SERVICE POINT
| <<A>> ALTERNATOR ASSEMBLY REMOVAL Remove the alternator assembly from above the vehicle.

[16] ENGINE ELECTRICAL - - CHARGING SYSTEM - ALTERNATOR ASSEMBLY - REMOVAL AND INSTALLATION <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation