[55A] HEATER, AIR CONDITIONER AND VENTILATION - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Item | Standard value
--- | ---
Idle speed r/min | 700 ± 100
Idle-up speed r/min | 850 ± 100
Resistor (for blower motor) Ω | LO | 2.54
ML | 1.24
MH | 0.6
Air gap (magnetic clutch) mm | 0.3 - 0.5

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation