[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ON-VEHICLE SERVICE - ACCELERATOR PEDAL POSITION SWITCH CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| ACCELERATOR PEDAL POSITION SWITCH CHECK
| Disconnect the accelerator pedal position sensor connector. Check continuity between terminal No. 4 (accelerator pedal position switch) and No. 5 (earth) of the connector.
Normal condition:
Accelerator pedal | Continuity
Depressed | No continuity
Released | Continuity (0 Ω)
| If defective, replace the accelerator pedal position sensor. NOTE: After replacement, adjust the accelerator pedal position sensor. (Refer to .)

[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ON-VEHICLE SERVICE - ACCELERATOR PEDAL POSITION SWITCH CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation