[55A] HEATER, AIR CONDITIONER AND VENTILATION - - ON-VEHICLE SERVICE - COMPRESSOR NOISE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

COMPRESSOR NOISE CHECK You must first know the conditions when the noise occurs. These conditions are: weather, vehicle speed, in gear or neutral, engine temperature or any other special conditions. Noises that develop during A/C operation can often be misleading. For example: what sounds like a failed front bearing or connecting rod, may be caused by loose bolts, nuts, mounting brackets, or a loose clutch assembly. Verify accessory drive belt tension (power steering or alternator). Improper accessory drive belt tension can cause a misleading noise when the compressor is engaged and little or no noise when the compressor is disengaged. Drive belts are speed-sensitive. That is, at different engine speeds, and depending upon belt tension, belts can develop unusual noises that are often mistaken for mechanical problems within the compressor.
ADJUSTMENT Select a quiet area for testing. Duplicate conditions as much as possible. Switch the compressor on and off several times to clearly identify compressor noise. To duplicate high ambient conditions (high head pressure), restrict air flow through the condenser. Install a manifold gauge set to make sure discharge pressure doesn't exceed 2,070 kPa. Tighten all compressor mounting bolts, clutch mounting bolt, and compressor drive belt. Check to assure clutch coil is tight (no rotation or wobble). Check refrigerant hoses for rubbing or interference that can cause unusual noises. Check refrigerant charge (Refer to ). Recheck compressor noise as in Step 1. If noise still exists, loosen compressor mounting bolts and retighten. Repeat Step 1. If noise continues, replace compressor and repeat Step 1.

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - ON-VEHICLE SERVICE - COMPRESSOR NOISE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation