[51] EXTERIOR - - GARNISHES - ADHESIVE | PRINT PAGE / INDEX / PRIOR / NEXT

GARNISHES

ADHESIVE
Application | Specified adhesive
--- | ---
Side sill garnish <2000> | Double-sided tape: A [5.0 mm width 0.8 mm thickness], B [5.0 mm width 1.2 mm thickness]
Side sill garnish <2400 (SPORT GEAR, GLS, GLX, XLS) > | Double-sided tape: [5.0 mm width 1.2 mm thickness]

[51] EXTERIOR - - GARNISHES - ADHESIVE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation