[1] PRE-DELIVERY INSPECTION - - ROAD TEST - 28. TRANSMISSION IN ALL RANGES | PRINT PAGE / INDEX / PRIOR / NEXT

| 28. TRANSMISSION IN ALL RANGES Manual transmission Check the transmission in all forward ranges and in reverse. Automatic transmission Make sure shift indicator lines up properly in all ranges. Depress the accelerator completely to check that the manual kickdown is operating correctly. Stop the vehicle on a steep incline. Put the automatic transmission in "P" position and slowly release the service brakes to see if "P" position lock holds. If it does not hold, the transmission requires further service.

[1] PRE-DELIVERY INSPECTION - - ROAD TEST - 28. TRANSMISSION IN ALL RANGES | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation