[23C] AUTOMATIC TRANSMISSION OVERHAUL <W5A5> - - PLANETARY CARRIER ASSEMBLY - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

PLANETARY CARRIER ASSEMBLY

DISASSEMBLY AND REASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Stopper plate
| >>B<< | 2. | One-way clutch
|  | 3. | Snap ring
|  | 4. | Output planetary carrier
| >>A<< | 5. | Thrust bearing No.3
|  | 6. | Underdrive sun gear
| >>A<< | 7. | Thrust bearing No.4
|  | 8. | Snap ring
|  | 9. | Overdrive planetary carrier
|  | 10. | Overdrive annulus gear
| REASSEMBLY SERVICE POINTS
| >>A<< THRUST BEARING No.4/No.3 INSTALLATION
| CAUTION Make sure the ends of each thrust bearing are oriented correctly. Install the thrust bearings No.4 and No.3 in position as shown in the illustration.
| >>B<< ONE-WAY CLUTCH INSTALLATION
| Insert the one-way clutch into the overdrive annulus gear with the arrow pointing to the output planetary carrier.

[23C] AUTOMATIC TRANSMISSION OVERHAUL <W5A5> - - PLANETARY CARRIER ASSEMBLY - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation