[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - CHECK AT ECU TERMINAL | PRINT PAGE / INDEX / PRIOR / NEXT

CHECK AT ECU TERMINAL
Terminal No. | Check item | Check conditions | Normal condition
--- | --- | --- | ---
15 | Throttle valve control servo relay | Ignition switch: "ON" | System voltage
Running at 3,500 r/min while engine is warming up after having been started. | 1 V or less
39 | Stop lamp switch | Ignition switch: "ON" | Depress the brake pedal. | System voltage
Release the brake pedal. | 1 V or less
51 | Inhibitor switch: "P" and "N" | Ignition switch: "ON" | Select lever: N or P range | System voltage
Select lever: Other than N or P range | 1 V or less
54 | Brake switch | Ignition switch: "ON" | Depress the brake pedal. | System voltage
Release the brake pedal. | 1 V or less
57 | Engine control relay | Ignition switch: "ON" | 1 V or less
Ignition switch: "LOCK" (OFF) | System voltage
58 | Engine-A/T-ECU backup power supply | Ignition switch: "LOCK" (OFF) | System voltage
92 | Accelerator pedal position sensor (main) power supply | Ignition switch: "ON" | 4.9 - 5.1 V
94 | Auto-cruise control switch power supply | Ignition switch: "ON" | All switches: OFF | 4.7 - 5.0 V
"CRUISE" (MAIN) switch: "ON" | 0 - 0.3 V
"COAST/SET" switch: ON | 2.0 - 2.8 V
"ACC/RES" switch: ON | 3.3 - 4.1 V
"CANCEL" switch: ON | 0.8 - 1.5 V
97 | Sensor impressed voltage | Ignition switch: "ON" | 4.9 - 5.1 V
106 | Throttle position sensor power supply | Ignition switch: "ON" | 4.9 - 5.1 V
107 | Accelerator pedal position sensor (sub) | Ignition switch: "ON" | Release the accelerator pedal | 0.335 - 0.935 V
Depress the accelerator pedal. | 4.0 V or more
113 | Throttle position sensor (sub) | Remove the intake air hose at the throttle body Disconnect the throttle position sensor, and then connect terminal numbers No. 3, No. 4, No. 5 and No. 6 with the use of the special tool (MB991658). Ignition switch: "ON" | Fully close the throttle valve with your finger | 2.2 - 2.8 V
Fully open the throttle valve with your finger | 4.6 V or more
114 | Accelerator pedal position sensor (main) | Ignition switch: "ON" | Release the accelerator pedal | 0.335 - 0.935 V
Depress the accelerator pedal. | 4.0 V or more
115 | Throttle position sensor (main) | Remove the intake air hose at the throttle body Disconnect the throttle position sensor, and then connect terminal numbers No. 3, No. 4, No. 5 and No. 6 with the use of the special tool (MB991658). Ignition switch: "ON" | Fully close the throttle valve with your finger | 0.3 - 0.7 V
Fully open the throttle valve with your finger | 4.0 V or more
132 | Engine-A/T-ECU power supply voltage applied to throttle valve control servo | Ignition switch: "ON" | System voltage

[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - CHECK AT ECU TERMINAL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation