[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - INPUT SIGNAL PROCEDURES - INSPECTION PROCEDURE P-10: The key reminder switch signal is not received. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE P-10: The key reminder switch signal is not received.
| CAUTION Whenever the ECU is replaced, ensure that the input signal circuit is normal.
| COMMENTS ON TROUBLE SYMPTOM Input signal from the key reminder switch is used to operate the functions below. If the signal is abnormal, these functions will not work normally. Ignition key reminder function Key reminder function Keyless entry system Ignition key cylinder illumination lamp Dome lamps
| POSSIBLE CAUSES Malfunction of the key reminder switch Malfunction of the ETACS-ECU Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Connector check: C-304 key reminder switch connector Q: Is the check result normal? YES: Go to Step 2. NO: Repair the connector.
| Step 2. Check the key reminder switch. Refer to GROUP 54A - Ignition switch . Q: Is the check result normal? YES: Go to Step 3. NO: Replace the key reminder switch.
| Step 3. Measure the resistance at the C-304 key reminder switch connector. Disconnect the connector, and measure at the wiring harness side. Resistance between C-304 key reminder switch connector terminal No.4 and body earth OK: 2 Ω or less Q: Is the check result normal? YES: Go to Step 5. NO: Go to Step 4.
| Step 4. Check the wiring harness between C-304 key reminder switch connector terminal No.4 and the body earth. Check the earth wires for open circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 5. Connector check: C-220 ETACS-ECU connector Q: Is the check result normal? YES: Go to Step 6. NO: Repair the connector.
| Step 6. Check the wiring harness between C-304 key reminder switch connector terminal No.6 and C-220 ETACS-ECU connector terminal No.30. Check the input line for open circuit. Q: Is the check result normal? YES: Go to Step 7. NO: Repair the wiring harness.
| Step 7. Retest the system. Check that the key reminder switch signal is received normally. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the ETACS-ECU.

[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - INPUT SIGNAL PROCEDURES - INSPECTION PROCEDURE P-10: The key reminder switch signal is not received. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation