[15] INTAKE AND EXHAUST - - INLET MANIFOLD - REMOVAL AND INSTALLATION <4G64-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G64-SOHC>
Pre-removal Operation Fuel Line Pressure Reduction [Refer to GROUP 13B, On-vehicle Service - Fuel Pump Connector Disconnection (How to Reduce Pressurized Fuel Lines) .] Engine Coolant Draining (Refer to GROUP 14, On-vehicle Service - Engine Coolant Replacement ). Air Cleaner Removal (Refer to ). Throttle Body Removal (Refer to GROUP 13B, Throttle Body ). Fuel Pressure Regulator, Delivery Pipe and Injector Assembly Removal (Refer to GROUP 13B, Injector ). | Post-installation Operation Fuel Pressure Regulator, Delivery Pipe and Injector Assembly Installation (Refer to GROUP 13B, Injector ). Throttle Body Installation (Refer to GROUP 13B, Throttle Body ). Air Cleaner Installation (Refer to ). Engine Coolant Refilling (Refer to GROUP 14, On-vehicle Service - Engine Coolant Replacement ). Accelerator Cable Adjustment (Refer to GROUP 17, On-vehicle Service - Accelerator Cable Check and Adjustment ). Fuel Leak Check
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Ignition coil connectors
|  | 2. | EGR control solenoid valve connector
|  | 3. | Detonation sensor connector
|  | 4. | Engine coolant temperature gauge unit connector
|  | 5. | Camshaft position sensor connector
|  | 6. | Engine coolant temperature sensor connector
|  | 7. | Capacitor connector
|  | 8. | Earth cable connection
|  | 9. | PCV hose connection
|  | 10. | Vacuum pipe <Vehicles with auto-cruise control>
|  | 11. | Vacuum hose and pipe assembly
|  | 12. | Solenoid valve assembly
|  | 13. | Brake booster vacuum hose connection
|  | 14. | Oil level gauge and guide
|  | 15. | O-ring
|  | 16. | Detonation sensor connector clamp
<<A>> | >>A<< | 17. | Radiator lower hose connection
|  | 18. | EGR valve
|  | 19. | EGR valve gasket
|  | 20. | Heater water hoses connection
|  | 21. | Thermostat case assembly
|  | 22. | O-ring
|  | 23. | Intake manifold stay
|  | 24. | Intake manifold assembly
|  | 25. | Intake manifold gasket
| REMOVAL SERVICE POINT
| <<A>> RADIATOR LOWER HOSE DISCONNECTION
| Make mating marks on the radiator hose and the hose clamp. Disconnect the radiator hose.
| INSTALLATION SERVICE POINT
| >>A<< RADIATOR LOWER HOSE CONNECTION
| Insert each hose as far as the projection of the water inlet fitting. Align the mating marks on the radiator hose and hose clamp, and then connect the radiator hose.

[15] INTAKE AND EXHAUST - - INLET MANIFOLD - REMOVAL AND INSTALLATION <4G64-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation