[27B] REAR AXLE <4WD> - - ON-VEHICLE SERVICE - GEAR OIL REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| GEAR OIL REPLACEMENT Remove the dynamic damper and filler plug. Remove the drain plug and drain oil. Tighten the drain plug to the specified torque. Tightening torque: 64 ± 4 N·m Add the oil until the level comes to the lower portion of the filler plug hole. Specified gear oil: Hypoid gear oil API classification GL-5 or higher Above 10°C: SAE 90 Below 10°C: SAE 80W Tighten the filler plug to the specified torque. Tightening torque: 49 ± 9 N·m Tighten the dynamic damper mounting nut to the specified torque. Tightening torque: 44 ± 9 N·m

[27B] REAR AXLE <4WD> - - ON-VEHICLE SERVICE - GEAR OIL REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation