[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - CRANKCASE EMISSION CONTROL SYSTEM - POSITIVE CRANKCASE VENTILATION (PCV) VALVE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| POSITIVE CRANKCASE VENTILATION (PCV) VALVE CHECK
| Insert a thin rod into the PCV valve from the side shown in the illustration (rocker cover installation side), and move the rod back and forth to check that the plunger moves. If the plunger does not move, there is a clogging in the PCV valve. In this case, clean or replace the PCV valve.

[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - CRANKCASE EMISSION CONTROL SYSTEM - POSITIVE CRANKCASE VENTILATION (PCV) VALVE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation