[23A] AUTOMATIC TRANSMISSION (FF) - - TRANSFER ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

TRANSFER ASSEMBLY

REMOVAL AND INSTALLATION
CAUTION * : Indicates parts which should be initially tightened, and then fully tightened after placing the vehicle horizontally and loading the full weight of the engine on the vehicle body.
Pre-removal and Post-installation Operation Under Cover Removal and Installation A/T fluid Draining and Supplying (Refer to GROUP 23A, On-vehicle Service ) Transfer Oil Draining and Supplying (Refer to GROUP 23A, On-vehicle Service .) Front Exhaust Pipe Removal and Installation (Refer to GROUP 15, Exhaust Pipe and Main Muffler .) Propeller Shaft Removal and Installation (Refer to GROUP 25.) Centremember Removal and Installation (Refer to GROUP 32, Engine Roll Stopper and Centremember .)
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Air guide
|  | • | Drive Shaft <RH> and Output Shaft Removal and Installation (Refer to GROUP 26, Drive Shaft Assembly .)
|  | 2. | Rear roll stopper connecting bolt
<<A>> |  | 3. | Transfer assembly
|  | 4. | O-ring
| REMOVAL SERVICE POINT
| <<A>> TRANSFER ASSEMBLY REMOVAL
| CAUTION After pulling out the transfer assembly, upon returning the transmission assembly to the original position be careful not to damage the bush parts of the roll stopper. Use a tyre lever, etc. to slide the transmission assembly to the front of the vehicle, create a clearance between the transmission assembly and crossmember, and then pull out the transfer assembly from that clearance.

[23A] AUTOMATIC TRANSMISSION (FF) - - TRANSFER ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation