[11F] ENGINE OVERHAUL <4G69> - - EXHAUST MANIFOLD - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

EXHAUST MANIFOLD

REMOVAL AND INSTALLATION
<Hong Kong>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Engine hanger
<<A>> | >>B<< | 2. | Oxygen sensor
<<A>> | >>B<< | 3. | Oxygen sensor
|  | 4. | Exhaust manifold cover
| >>A<< | 5. | Exhaust manifold bracket B
|  | 6. | Exhaust manifold
|  | 7. | Exhaust manifold gasket
|  | 8. | Exhaust manifold bracket A
<Except Hong Kong>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Engine hanger
|  | 2. | Exhaust manifold cover
|  | 3. | Exhaust manifold
|  | 4. | Exhaust manifold gasket
| REMOVAL SERVICE POINT
| <<A>> OXYGEN SENSOR REMOVE
| Using special tool Oxygen sensor wrench (MD998770), removal the oxygen sensor.
| INSTALLATION SERVICE POINT
| >>A<< EXHAUST MANIFOLD BRACKET "B" INSTALLATION
| Check to ensure that the exhaust manifold bracket "B" is in close contact with the exhaust manifold and the cylinder block before tightening the respective mounting bolts to the specified torque.
| >>B<< OXYGEN SENSOR INSTALLATION
| Using special tool Oxygen sensor wrench (MD998770), installation the oxygen sensor.

[11F] ENGINE OVERHAUL <4G69> - - EXHAUST MANIFOLD - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation