[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - INJECTOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

INJECTOR

REMOVAL AND INSTALLATION
Pre-removal Operation Fuel Discharge Prevention (Refer to ). Air Cleaner Removal (Refer to GROUP 15, Air Cleaner ). | Post-installation Operation Air Cleaner Installation (Refer to GROUP 15, Air Cleaner ). Fuel Leakage Inspection.
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | PCV hose connection
|  | 2. | Capacitor connector
|  | 3. | Ignition coil connector
|  | 4. | Injector connector
|  | 5. | EGR valve connector
|  | 6. | Rocker cover bracket installation bolts
| >>A<< | 7. | Fuel high-pressure hose connection
|  | 8. | O-ring
<<A>> |  | 9. | Fuel delivery pipe and fuel injector assembly
|  | 10. | Insulators
| >>A<< | 11. | Fuel injector assembly
|  | 12. | Fuel delivery pipe
|  | 13. | O-ring
|  | 14. | Insulators
|  | 15. | Grommets
|  | 16 | Fuel injectors
| REMOVAL SERVICE POINT
| <<A>> FUEL DELIVERY PIPE AND FUEL INJECTOR ASSEMBLY REMOVAL CAUTION Do not drop the injector. Remove the fuel delivery pipe with the fuel injector assembly attached to it.
| INSTALLATION SERVICE POINT
| >>A<< FUEL INJECTOR ASSEMBLY/FUEL HIGH-PRESSURE HOSE INSTALLATION CAUTION Do not let the engine oil get into the delivery pipe will be damaged. Apply a drop of new engine oil to the O-ring. Turn the fuel injector assembly to the right and left to install to the fuel delivery pipe. Repeat for fuel high-pressure hose. Be careful not to damage the O-ring. After installing, check that the item turns smoothly. If it dose not turn smoothly, the O-ring may be trapped, remove the item, re-install it into the fuel delivery pipe and check again. Tighten the fuel high-pressure hose to the specified torque. Tightening torque: 5.0 ± 1.0 N·m

[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - INJECTOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation