[0] GENERAL - - PRECAUTIONS BEFORE SERVICE - PARTS TO BE REPLACED | PRINT PAGE / INDEX / PRIOR / NEXT

| PARTS TO BE REPLACED
| If any of the following parts are removed, they must be replaced with new parts. Oil seals Gaskets (except rocker cover gasket) Packings O-rings Lock washers Split pins Self-locking nuts

[0] GENERAL - - PRECAUTIONS BEFORE SERVICE - PARTS TO BE REPLACED | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation