[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - POWER WINDOWS - INSPECTION PROCEDURE D-4: Front and/or rear passenger's power window(s) do not work by means of the power window main switch. <LH drive vehicles for Argentina> | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE D-4: Front and/or rear passenger's power window(s) do not work by means of the power window main switch. <LH drive vehicles for Argentina>
| COMMENTS ON TROUBLE SYMPTOM If the passenger's and/or rear power window does not work by means of the power window main switch, the power window main switch or the respective power window sub switch(es) may be defective.
| POSSIBLE CAUSES Malfunction of the power window main switch Malfunction of the power window sub switch (front RH), power window sub switch (rear RH) or power window sub switch (rear LH) Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Check the power window main switch. Check that the driver's power window works by means of the power window main switch. Q: Is the check result normal? YES: Go to Step 2. NO: Refer to Inspection Procedure D-2 "Driver's power window does not work by means of the power window main switch <Vehicles for Argentina>."
| Step 2. Check the power window sub switch. Check that each power window works by means of the respective power window sub switch when the power window lock switch is turned off. Q: Is the check result normal? YES: Go to Step 3. NO: Refer to Inspection Procedure D-3 "Relevant power window(s) do not work by means of the front and rear passenger's power window sub switches <LH drive vehicles for Argentina>."
| Step 3. Determine a trouble spot. Q: Which power window does not work when the power window main switch is operated? Front passenger's door: Go to Step 4. Rear right door: Go to Step 7. Rear left door: Go to Step 10.
| Step 4. Connector check: E-05 power window main switch connector and E-17 power window sub switch (front RH) connector Q: Is the check result normal? YES: Go to Step 5. NO: Repair the connector.
| Step 5. Check the wiring harness between E-05 power window main switch connector terminal No.11 and E-17 power window sub switch (front LH) connector terminal No.6. NOTE: Prior to the wiring harness inspection, check intermediate connectors C-15, C-118, E-12 and E-24, and repair if necessary. Check the communication lines for open circuit. Q: Is the check result normal? YES: Go to Step 6. NO: Repair the wiring harness.
| Step 6. Retest the system. After the power window sub switch (front LH) is replaced, check that the front passenger's door power window can be operated by the power window sub switch. Replace the power window sub switch (front LH). Check that the front passenger's power window works by means of the power window main switch. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the power window main switch.
| Step 7. Connector check: E-05 power window main switch connector and E-21 power window sub switch (rear RH) connector Q: Is the check result normal? YES: Go to Step 8. NO: Repair the connector.
| Step 8. Check the wiring harness between E-05 power window main switch connector terminal No.11 and E-21 power window sub switch (rear RH) connector terminal No.6. NOTE: Prior to the wiring harness inspection, check intermediate connectors C-13, C-118, D-02, E-12 and E-27, and repair if necessary. Check the communication lines for open circuit. Q: Is the check result normal? YES: Go to Step 9. NO: Repair the wiring harness.
| Step 9. Retest the system. After the power window sub switch (rear RH) is replaced, check that the rear right door power window can be operated by the power window sub switch. Replace the power window sub switch (rear RH). Check that the rear right power window works by means of the power window main switch. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the power window main switch.
| Step 10. Connector check: E-05 power window main switch connector and E-01 power window sub switch (rear LH) connector Q: Is the check result normal? YES: Go to Step 11. NO: Repair the connector.
| Step 11. Check the wiring harness between E-05 power window main switch connector terminal No.11 and E-01 power window sub switch (rear LH) connector terminal No.6. NOTE: Prior to the wiring harness inspection, check intermediate connectors C-117, C-118, D-26, E-09 and E-12, and repair if necessary. Check the communication lines for open circuit. Q: Is the check result normal? YES: Go to Step 12. NO: Repair the wiring harness.
| Step 12. Retest the system. After the power window sub switch (rear LH) is replaced, check that the rear left door power window can be operated by the power window sub switch. Replace the power window sub switch (rear LH). Check that the rear left power window works by means of the power window main switch. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the power window main switch.

[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - POWER WINDOWS - INSPECTION PROCEDURE D-4: Front and/or rear passenger's power window(s) do not work by means of the power window main switch. <LH drive vehicles for Argentina> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation