[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - ON-VEHICLE SERVICE - IN THE EVENT OF A DISCHARGED BATTERY | PRINT PAGE / INDEX / PRIOR / NEXT

| IN THE EVENT OF A DISCHARGED BATTERY WARNING If the ABS is not operating, the vehicle posture will be unstable during braking, Do not drive the vehicle with the ABS-ECU connector disconnected or with the ABS not operating for any other reason. If the engine is started using a booster cable when the battery is completely flat, and the vehicle is then driven without waiting for the battery to be recharged, the engine may misfire and it may not be possible to drive the vehicle. This is because the ABS consumes a large amount of current when carrying out its initial checks. If this happens, recharge the battery fully.

[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - ON-VEHICLE SERVICE - IN THE EVENT OF A DISCHARGED BATTERY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation