[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - INPUT SIGNAL PROCEDURES - INSPECTION PROCEDURE P-19: The rear fog lamp switch signal is not received. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE P-19: The rear fog lamp switch signal is not received.
| CAUTION Whenever the ECU is replaced, ensure that the input signal circuit is normal.
| COMMENTS ON TROUBLE SYMPTOM Input signal from the fog lamp switch is used to operate the rear fog lamps. If the signal is abnormal, the rear fog lamps will not illuminate and extinguish normally.
| POSSIBLE CAUSES Malfunction of the fog lamp switch Malfunction of the ETACS-ECU Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Connector check: C-03 fog lamp switch connector Q: Is the check result normal? YES: Go to Step 2. NO: Repair the defective connector.
| Step 2. Check the rear fog lamp switch. Refer to GROUP 54A - Rear fog lamp . Q: Is the check result normal? YES: Go to Step 3. NO: Replace the fog lamp switch.
| Step 3. Resistance measurement at the C-03 fog lamp switch connector. Remove the fog lamp switch, and measure at the wiring harness side. Continuity between C-03 fog lamp switch connector terminal No.2 and body earth OK: 2Ω or less Q: Is the check result normal? YES: Go to Step 5. NO: Go to Step 4.
| Step 4. Check the wiring harness between C-03 fog lamp switch connector terminal No.2 and body earth. Check the earth wires for open circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 5. Connector check: C-35 rear fog lamp-ECU connector Q: Is the check result normal? YES: Go to Step 6. NO: Repair the defective connector.
| Step 6. Check the wiring harness between C-35 rear fog lamp-ECU connector terminal No.6 and C-03 fog lamp switch connector terminal No.1. Check the input line for open circuit. Q: Is the check result normal? YES: Go to Step 7. NO: Repair the wiring harness.
| Step 7. Retest the system. Check that the rear fog lamp switch signal is received normally. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the ETACS-ECU.

[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - INPUT SIGNAL PROCEDURES - INSPECTION PROCEDURE P-19: The rear fog lamp switch signal is not received. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation