[00] GENERAL - - GENERAL DATA AND SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL DATA AND SPECIFICATIONS
VEHICLES FOR GENERAL EXPORT (Except for Hong Kong spec., Brazil, South Africa and Argentina)
Items | CU4W | CU5W
--- | --- | ---
XRHEZL/R | XRMYZL | XRHYZL | XRHJZL
Vehicle dimensions mm | Front track | 1 | 1,495
Overall width | 2 | 1,780 | 1,750 | 1,780
Front overhang | 3 | 945
Wheel base | 4 | 2,625
Rear overhang | 5 | 975
Overall length | 6 | 4,545
Ground clearance (unladen) | 7 | 205
Overall height (unladen) | 8 | 1,630/1,680*1
Rear track | 9 | 1,505
Vehicle weight kg | Kerb weight | 1,530 | 1,530 | 1,535 | 1,550
Max. gross vehicle weight | 2,000
Max. axle weight rating-front | 1,050
Max. axle weight rating-rear | 1,065
Seating capacity | 5
Engine | Model No. | 4G64 | 4G69
Total displacement mL | 2,351 | 2,378
Transmission | Model No. | W4A42 | W4A4B
Type | 4-speed automatic
Fuel system | Fuel supply system | MPI | MPI MIVEC
NOTE: *1 : Vehicles with roof rails
(For Hong Kong spec.)
Items | CU2W | CU5W
--- | --- | ---
LRMER1D | LYXFZR1D | XRHYZR1D
Vehicle dimensions mm | Front track | 1 | 1,495
Overall width | 2 | 1,750 | 1,780
Front overhang | 3 | 900 | 950
Wheel base | 4 | 2,625
Rear overhang | 5 | 940 | 975
Overall length | 6 | 4,465 | 4,550
Ground clearance (unladen) | 7 | 195 | 160 | 205
Overall height (unladen) | 8 | 1,550/1,585*1 | 1,540/1,575*1 | 1,685
Rear track | 9 | 1,495 | 1,505
Vehicle weight kg | Kerb weight | 1,363 | 1,533 | 1,523
Max. gross vehicle weight | 1,690 | 1,860 | 1,840
Max. axle weight rating-front | 950 | 1,050 | 1,020
Max. axle weight rating-rear | 740 | 810 | 820
Seating capacity | 5
Engine | Model No. | 4G63-SOHC | 4G63-DOHC | 4G69
Total displacement mL | 1,997 | 1,997 | 2,378
Transmission | Model No. | W4A42 | W5A51 | W4A4B
Type | 4-speed automatic | 5-speed automatic | 4-speed automatic
Fuel system | Fuel supply system | MPI | MPI MIVEC
NOTE: *1 : Vehicles with roof rails
(For Brazil)
Items | CU5W
--- | ---
XRMYZL1F | XRHYZL1F
Vehicle dimensions mm | Front track | 1 | 1,495
Overall width | 2 | 1,750/1,780*1
Front overhang | 3 | 945
Wheel base | 4 | 2,625
Rear overhang | 5 | 975
Overall length | 6 | 4,545
Ground clearance (unladen) | 7 | 205
Overall height (unladen) | 8 | 1,630/1,680*2
Rear track | 9 | 1,505
Vehicle weight kg | Curb weight | 1,545 | 1,550
Max. gross vehicle weight | 2,000
Max. axle weight rating-front | 1,050
Max. axle weight rating-rear | 1,065
Seating capacity | 5
Engine | Model No. | 4G69
Total displacement mL | 2,378
Transmission | Model No. | W4A4B
Type | 4-speed automatic
Fuel system | Fuel supply system | MPI MIVEC
NOTE: *1 : Vehicles with over fender NOTE: *2 : Vehicles with roof rails
(For South Africa and Argentina)
Items | CU5W
--- | ---
XRMYZR6S | XRHYZR6S | XRHYZL6A
Vehicle dimensions mm | Front track | 1 | 1,495
Overall width | 2 | 1,750 | 1,780
Front overhang | 3 | 945
Wheel base | 4 | 2,625
Rear overhang | 5 | 975
Overall length | 6 | 4,545
Ground clearance (unladen) | 7 | 195
Overall height (unladen) | 8 | 1,620/1,670*1 | 1,670
Rear track | 9 | 1,505
Vehicle weight kg | Curb weight | 1,560 | 1,565
Max. gross vehicle weight | 2,070
Max. axle weight rating-front | 1,050
Max. axle weight rating-rear | 1,065
Seating capacity | 5
Engine | Model No. | 4G69
Total displacement mL | 2,378
Transmission | Model No. | W4A4B
Type | 4-speed automatic
Fuel system | Fuel supply system | MPI MIVEC
NOTE: *1 : Vehicles with roof rails
Vehicles for GCC
Items | CU5W
--- | ---
XRMYZLW | XRHYZLW
Vehicle dimensions mm | Front track | 1 | 1,495
Overall width | 2 | 1,750 | 1,780
Front overhang | 3 | 945
Wheel base | 4 | 2,625
Rear overhang | 5 | 975
Overall length | 6 | 4,545
Ground clearance (unladen) | 7 | 205
Overall height (unladen) | 8 | 1,680
Rear track | 9 | 1,505
Vehicle weight kg | Kerb weight | 1,535 | 1,545
Max. gross vehicle weight | 2,000
Max. axle weight rating-front | 1,050
Max. axle weight rating-rear | 1,065
Seating capacity | 5
Engine | Model No. | 4G69
Total displacement mL | 2,378
Transmission | Model No. | W4A4B
Type | 4-speed automatic
Fuel system | Fuel supply system | MPI MIVEC
VEHICLES FOR NEW ZEALAND
Items | CU2W | CU5W
--- | --- | ---
LRMER1D | LYXFZR1D | XRMYZR8 | XRHYZR8 | XRXYZR8
Vehicle dimensions mm | Front track | 1 | 1,495 | 1,510
Overall width | 2 | 1,750 | 1,780
Front overhang | 3 | 900 | 950
Wheel base | 4 | 2,625
Rear overhang | 5 | 940 | 975
Overall length | 6 | 4,465 | 4,550
Ground clearance | 7 | 195 | 160 | 205
Overall height | 8 | 1,550/1,585*1 | 1,540/1,575*1 | 1,630/1,680*1
Rear track | 9 | 1,495 | 1,505 | 1,520
Vehicle weight kg | Kerb weight | 1,363 | 1,533 | 1,560 | 1,580 | 1,575
Max. gross vehicle weight | 1,690 | 1,860 | 2,000
Max. axle weight rating-front | 950 | 1,050 | 1,050
Max. axle weight rating-rear | 740 | 810 | 1,065
Seating capacity | 5
Engine | Model No. | 4G63-SOHC | 4G63-DOHC | 4G69
Total displacement mL | 1,997 | 1,997 | 2,378
Transmission | Model No. | W4A42 | W5A51 | W4A4B
Type | 4-speed automatic | 5-speed automatic | 4-speed automatic
Fuel system | Fuel supply system | MPI | MPI MIVEC
NOTE: *1 : Vehicles with roof rails
Vehicles for Australia
Items | CU5W
--- | ---
XRMYZR8 | XRHYZR8 | XRXYZR8
Vehicle dimensions mm | Front track | 1 | 1,495 | 1,510
Overall width | 2 | 1,750 | 1,780
Front overhang | 3 | 950
Wheel base | 4 | 2,625
Rear overhang | 5 | 975
Overall length | 6 | 4,550
Ground clearance | 7 | 205
Overall height | 8 | 1,630/1,680*1
Rear track | 9 | 1,505 | 1,520
Vehicle weight kg | Kerb weight | 1,560 | 1,580 | 1,575
Max. gross vehicle weight | 2,000
Max. axle weight rating-front | 1,050
Max. axle weight rating-rear | 1,065
Seating capacity | 5
Engine | Model No. | 4G69
Total displacement mL | 2,378
Transmission | Model No. | W4A4B
Type | 4-speed automatic
Fuel system | Fuel supply system | MPI MIVEC
NOTE: *1 : Vehicles with roof rails

[00] GENERAL - - GENERAL DATA AND SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation