[15] INTAKE AND EXHAUST - - EXHAUST MANIFOLD AND TURBOCHARGER - TURBOCHARGER ASSEMBLY CHECK (DISASSEMBLY AND REASSEMBLY) | PRINT PAGE / INDEX / PRIOR / NEXT

TURBOCHARGER ASSEMBLY CHECK (DISASSEMBLY AND REASSEMBLY)
| TURBINE HOUSING
| Check the turbine housing for turbine wheel contact marks, cracks due to overheating, pitting, deformation, or other kinds of damage. Replace the turbine housing if any crack is found. Operate the waste gate valve lever by hand to check that the valve can be opened and closed smoothly.
| COMPRESSOR COVER Check the compressor cover for compressor wheel contact marks or other damage.
| CARTRIDGE ASSEMBLY
| Check the vanes of the turbine and compressor wheel for deformation, damage on edges and other surfaces, corrosion, contact marks on back surfaces, and any other defect. Replace the cartridge assembly if any of the defects is present in the vanes. Check the oil and coolant passages for clogging and damage.
| WASTE GATE ACTUATOR
| CAUTION Never apply a pressure greater than 113.3 kPa. Applying a higher pressure could result in a broken diaphragm. Check that the rod moves when a pressure of the standard value is applied to the actuator using a tester. Standard value: 100 kPa

[15] INTAKE AND EXHAUST - - EXHAUST MANIFOLD AND TURBOCHARGER - TURBOCHARGER ASSEMBLY CHECK (DISASSEMBLY AND REASSEMBLY) | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation