[52A] INTERIOR - - FRONT SEAT BELT - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

FRONT SEAT BELT

REMOVAL AND INSTALLATION CAUTION SRS: Before removing and installing the seat belts with pre-tensioner, refer to GROUP 52B, Seat Belt with Pre-tensioner .
Pre-removal and Post-installation Operation Turn the ignition key to the LOOK (OFF) position. Disconnect the negative battery terminal.
|  |  | Outer seat belt removal steps
--- | --- | --- | ---
|  | 1. | Sash guide cover
|  | • | Centre pillar trim lower (Refer to ).
|  | 2. | Bracket
|  | 3. | Outer seat belt (Refer to GROUP 52B, Seat Belt with Pre-tensioner ).
|  | 4. | Centre pillar trim upper (Refer to ).
|  | 5. | Adjustable seat belt anchor
|  |  | Inner seat belt removal steps
|  | 6. | Harness connector (Driver’s side) <Vehicles for GCC, Hong Kong and Australia>
|  | • | Shield cover (Refer to ).
|  | 7. | Inner seat belt

[52A] INTERIOR - - FRONT SEAT BELT - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation