[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - ON-VEHICLE SERVICE - ENGINE COOLANT TEMPERATURE SENSOR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| ENGINE COOLANT TEMPERATURE SENSOR CHECK CAUTION Be careful not to touch the connector (resin section) with the tool when removing and installing.
| Remove the engine coolant temperature sensor.
| With temperature sensing portion of engine coolant temperature sensor immersed in hot water, check resistance. Standard value: 14 - 17 kΩ (at -20°C) 5.1 - 6.5 kΩ (at 0°C) 2.1 - 2.7 kΩ (at 20°C) 0.9 - 1.3 kΩ (at 40°C) 0.48 - 0.68 kΩ (at 60°C) 0.26 - 0.36 kΩ (at 80°C) If the resistance deviates from the standard value greatly, replace the sensor.
| Apply sealant to threaded portion. Specified sealant: 3M NUT Locking Part No. 4171 or equivalent Install the engine coolant temperature sensor and tighten it to the specified torque. Tightening torque: 29 ± 10 N·m

[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - ON-VEHICLE SERVICE - ENGINE COOLANT TEMPERATURE SENSOR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation