[11B] ENGINE OVERHAUL <4G6-SOHC> - - ALTERNATOR AND IGNITION SYSTEM - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

ALTERNATOR AND IGNITION SYSTEM

REMOVAL AND INSTALLATION
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Auto tensioner
|  | 2. | Water pump pulley
|  | 3. | Alternator brace
|  | 4. | Alternator
|  | 5. | Crankshaft pulley
|  | 6. | Spark plug cable
|  | 7. | Ignition coil
|  | 8. | Spark plug
|  | 9. | Camshaft position sensor
| >>A<< | 10. | Camshaft position sensor support
|  | 11. | Camshaft position sensing cylinder
| INSTALLATION SERVICE POINTS
| >>A<< CAMSHAFT POSITION SENSOR SUPPORT INSTALLATION
| Apply a 3mm diameter bead of form-in-place gasket (FIPG) to the gasket surface as shown in the drawing. Specified sealant: Mitsubishi Genuine Part No.MD970389 or equivalent

[11B] ENGINE OVERHAUL <4G6-SOHC> - - ALTERNATOR AND IGNITION SYSTEM - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation