[11B] ENGINE MECHANICAL <4G6-DOHC> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION The 4G63-DOHC-T/C engine have been adopted in the new OUTLANDER.
MAJOR SPECIFICATIONS
Item | 4G63-DOHC-T/C
--- | ---
Total displacement mL | 1,997
Combustion chamber | Pent roof type
Bore × Stroke mm | 85.0 × 88.0
Compression ratio | 8.8
Camshaft-valve arrangement | DOHC-16valves
Valve timing | Intake opening | BTDC 17°
Intake closing | ABDC 51°
Exhaust opening | BBDC 57°
Exhaust closing | ATDC 15°
Maximum output kW (PS) /rpm | 169(230) /5,500
Maximum torqe Nm/rpm | 343/3,000
Lash adjuster | Equipped

[11B] ENGINE MECHANICAL <4G6-DOHC> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation