[27B] REAR AXLE <4WD> - - REAR AXLE HUB ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| WHEEL BEARING ROTATION STARTING TORQUE AND AXIAL PLAY CHECK
| Tighten the following special tools to the specified torque. Spacer (MB991000) Front hub remover and installer (MB991017) Rotate the rear hub in order to seat the bearing.
| Measure the wheel bearing rotation starting torque by using the following special tools. Preload socket (MB990326) Torque wrench (MB990685) Limit: 1.0 N·m The rotation starting torque must be within the limit and wheel bearing must rotate smoothly.
| Measure to determine whether the wheel bearing axial play is within the specified limit or not. Limit: 0.05 mm If the play is not within the limit range while the nut is tightened to 245 ± 29 N·m, the bearing, trailing arm and/or rear hub have probably not been installed correctly. Replace the bearing and re-install.

[27B] REAR AXLE <4WD> - - REAR AXLE HUB ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation