[52A] INTERIOR - - DOOR TRIM - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

DOOR TRIM

REMOVAL AND INSTALLATION
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Speaker garnish
<<A>> |  | 2. | Door inside handle cover
|  | • | Delta cover (Refer to GROUP 51, Door Mirror ).
|  | 3. | Door trim assembly
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Speaker garnish
<<A>> |  | 2. | Door inside handle cover
|  | 3. | Door trim assembly
| REMOVAL SERVICE POINT
| <<A>> DOOR INSIDE HANDLE COVER REMOVAL
| Insert a flat-tipped screwdriver into the back end of the tapping screw cap of the door inside handle cover. Try the screwdriver in the direction of the arrow. Remove the cap, then remove the tapping screw.
| Insert a special tool ornament remover (MB990784) in the gap between the door inside handle cover and door inside handle in the area shown. Then remove the thumb clamp of the door inside handle cover and door inside handle. Insert a special tool from the back end of the door inside handle cover to lift it in the direction of the arrow. Then remove the door inside handle cover.

[52A] INTERIOR - - DOOR TRIM - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation