[35A] BASIC BRAKE SYSTEM - - REAR DRUM BRAKE - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

REAR DRUM BRAKE

REMOVAL AND INSTALLATION
Pre-removal Operation Loosening the Parking Brake Cable Adjusting Nut (Refer to GROUP 36, On-vehicle Service - Parking Brake Lever Stroke Check and Adjustment ). <LH drive vehicles> Loosening the Parking Brake Cable Adjusting Nut (Refer to GROUP 36, On-vehicle Service - Parking Brake Pedal Stroke Check and Adjustment ). <RH drive vehicles> Brake Fluid Draining | Post-installation Operation Brake Fluid Filling and Air Bleeding (Refer to ). Parking Brake Lever Stroke Adjustment (Refer to GROUP 36, On-vehicle Service - Parking Brake Lever Stroke Check and Adjustment ). <LH drive vehicles> Parking Brake Pedal Stroke Adjustment (Refer to GROUP 36, On-vehicle Service - Parking Brake Pedal Stroke Check and Adjustment ). <RH drive vehicles>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Brake drum
<<A>> |  | 2. | Parking brake cable connection
|  | 3. | Shoe-to-shoe spring
|  | 4. | Adjuster lever
|  | 5. | Auto adjuster assembly
|  | 6. | Retainer spring
|  | 7. | Shoe hold-down cup
|  | 8. | Shoe hold-down spring
|  | 9. | Shoe-to-lever spring
|  | 10. | Shoe and lining assembly
|  | 11. | Shoe and lever assembly
<<B>> | >>B<< | 12. | Retainer
| >>A<< | 13. | Wave washer
|  | 14. | Parking lever
|  | 15. | Shoe and lining assembly
|  | 16. | Shoe hold-down pin
|  | 17. | Brake pipe connection
|  | 18. | Wheel cylinder assembly
|  | 19. | Lock nut
|  | 20. | Rear hub assembly [Refer to GROUP 34, Trailing arm assembly <2WD> or <4WD>].
|  | 21. | Backing plate
| REMOVAL SERVICE POINTS
| <<A>> PARKING BRAKE CABLE CONNECTION REMOVAL
| Withdraw the parking brake cable from the backing plate. NOTE: Insert a 10 mm-wrench into the parking brake cable to facilitate the cable withdrawal.
| <<B>> RETAINER REMOVAL
| Use a flat-tipped screwdriver or a similar tool to open up the retainer joint. Then remove the retainer.
| INSTALLATION SERVICE POINTS
| >>A<< WAVE WASHER INSTALLATION
| Install the wave washer in the direction shown in the illustration.
| >>B<< RETAINER INSTALLATION
| Use pliers or a similar tool to close the retainer end onto the pin.

[35A] BASIC BRAKE SYSTEM - - REAR DRUM BRAKE - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation