[1] PRE-DELIVERY INSPECTION - - ROAD TEST - 32. ELECTRICAL EQUIPMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| 32. ELECTRICAL EQUIPMENT
| Radio Tune the radio to a local broadcasting station and check the following: Operate the volume, tone, balance and fader controls, etc. Pull out the pushbuttons, dial another station and set each pushbuttons. Operate the AM/FM switch. Tape player Insert a cassette tape in the tape player and check as follows: Check the operation of the tape feeder and rewind. Check the ejection. Check the operation of volume, tone, balance and fader controls, etc.

[1] PRE-DELIVERY INSPECTION - - ROAD TEST - 32. ELECTRICAL EQUIPMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation