[42] BODY - - SECURITY ALARM <Vehicles for Hong Kong spec> - ON-VEHICLE SERVICE - SECURITY ALARM FUNCTION CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| ON-VEHICLE SERVICE

| SECURITY ALARM FUNCTION CHECK Check that the security alarm works. If the alarm does not work, carry out troubleshooting. Refer to GROUP 54B, Troubleshooting , refer to GROUP 54C, Troubleshooting . NOTE: The adjustment function allows you to change the security alarm setting from "without function (initial setting)" to "alarm by horns and hazard warning lamps" or "alarm by hazard warning lamps only". Prior to that check, confirm which setting is activated.

[42] BODY - - SECURITY ALARM <Vehicles for Hong Kong spec> - ON-VEHICLE SERVICE - SECURITY ALARM FUNCTION CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation