[42] BODY - - SUNROOF ASSEMBLY - SUNROOF ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| SUNROOF SWITCH CONTINUITY CHECK
SWITCH POSITION | TESTER CONNECTION | SPECIFIED CONDITION
--- | --- | ---
Open | 4 - 5 | Less than 2 ohms
OFF | 3 - 4, 3 - 5, 3 - 6, 4 - 5, 4 - 6, 5 - 6 | Open circuit
Up | 3 - 4 | Less than 2 ohms
Close/Down | 4 - 6 | Less than 2 ohms

[42] BODY - - SUNROOF ASSEMBLY - SUNROOF ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation