[42] BODY - - SUNROOF ASSEMBLY - ON-VEHICLE SERVICE - SUNROOF SAFETY FUNCTION CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| SUNROOF SAFETY FUNCTION CHECK Close the roof lid glass by applying an approximately 10mm thickness wood chip placed at a right angle to the roof lid glass. Check to see if the roof lid glass opens after the motor turns when the roof lid glass catches the wooden chip. Refer to GROUP 54B, Troubleshooting , refer to GROUP 54C, Troubleshooting , refer to GROUP 54D, Troubleshooting or refer to GROUP 54E, Troubleshooting .

[42] BODY - - SUNROOF ASSEMBLY - ON-VEHICLE SERVICE - SUNROOF SAFETY FUNCTION CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation