[13D] FUEL SUPPLY - - ON-VEHICLE SERVICE - FUEL TANK PUMP AND GAUGE ASSEMBLY REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| FUEL TANK PUMP AND GAUGE ASSEMBLY REPLACEMENT Remove the rear seat cushion assembly (Refer to GROUP 52A - Rear Seat Assembly ).
| Remove the service hole cover mounting screws and remove the service hole cover.
| Disconnect the fuel assembly <2WD> or fuel tank pump and gauge assembly <4WD> connector, fuel tank differential pressure sensor connector <Vehicles for Brazil and Chile>, fuel return hose <Except for 4G69>, fuel high-pressure hose and fuel suction tube <4WD>.
| CAUTION For 4WD:Pay attention not to damage the float when removing and installing fuel tank pump and gauge assembly through the service hole. Remove the mounting nuts and fuel pump bracket plate, and remove the fuel pump assembly <2WD>, fuel tank pump and gauge assembly <4WD> from the service hole. Install the fuel pump assembly <2WD>, fuel tank pump and gauge assembly <4WD> to the fuel tank through the service hole.
| Install the fuel pump bracket plate to the fuel tank and tighten the mounting nuts to the specified torque. Tightening torque: 2.5 ± 0.4 N·m
| CAUTION After connecting the fuel high-pressure hose or fuel pump suction tube, slightly pull it to ensure that it is installed securely. Also confirm that there is a play approximately 3 mm.
| Connect the fuel pump assembly <2WD> fuel tank pump and gauge assembly <4WD> connector, fuel tank differential pressure sensor connector <Vehicles for Brazil and Chile>, fuel return hose, fuel high-pressure hose and fuel suction tube <4WD>.
| Tighten the service hole cover mounting screws and install the service hole cover. Install the rear seat cushion assembly (Refer to GROUP 52A - Rear Seat Assembly ).

[13D] FUEL SUPPLY - - ON-VEHICLE SERVICE - FUEL TANK PUMP AND GAUGE ASSEMBLY REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation