[34] REAR SUSPENSION - - TRAILING ARM ASSEMBLY - TRAILING ARM BUSHING REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| TRAILING ARM BUSHING REPLACEMENT
| Use following special tools to drive out the trailing arm bushing. MB991444: Bushing Remover and Installer Arbor MB991445: Bushing Remover and Installer Base
| Set the installation direction and installation location of the trailing arm bushing. Place the long projection end of the trailing arm bushing inner pipe towards the inside of the vehicle. Make sure that the hollow of the trailing arm bushing is located as shown in the illustration.
| Using the special tools, press the trailing arm bushing into the position shown.

[34] REAR SUSPENSION - - TRAILING ARM ASSEMBLY - TRAILING ARM BUSHING REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation