[54A] CHASSIS ELECTRICAL - - SPEED ALARM SYSTEM <VEHICLES FOR GCC> | PRINT PAGE / INDEX / PRIOR / NEXT

SPEED ALARM SYSTEM <VEHICLES FOR GCC> The speed alarm-ECU sounds the speed alarm buzzer when the vehicle speed reaches 120 ± 5 km/h. The ECU monitors vehicle speed signal from the engine-A/T-ECU to sound the buzzer.
CONSTRUCTION DIAGRAM
SYSTEM BLOCK DIAGRAM

[54A] CHASSIS ELECTRICAL - - SPEED ALARM SYSTEM <VEHICLES FOR GCC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation