[51] EXTERIOR - - FRONT BUMPER ASSEMBLY - FRONT BUMPER ASSEMBLY - DISASSEMBLY AND REASSEMBLY <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

DISASSEMBLY AND REASSEMBLY <2400>
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Licence plate garnish
|  | 2. | Centre cover
<<A>> | >>A<< | 3. | Rivets A
<<A>> | >>A<< | 4. | Rivets B
|  | 5. | Front bumper side plate
|  | 6. | Front bumper centre reinforcement
|  | 7. | Oil cooler duct
|  | 8. | Air intake bezel (Vehicles without fog lamp)
|  | 9. | Fog lamp bezel
|  | 10. | Fog lamp assembly
|  | 11. | Front bumper core
|  | 12. | Three-diamond mark
|  | 13. | Front bumper extension <SPORT GEAR, GLS, GLX, XLS>
|  | 14. | Front bumper face
| DISASSEMBLY SERVICE POINT
| <<A>> RIVETS A / RIVETS B REMOVAL
| Use a drill (&phis;4.0 mm) to make a hole in the rivet to break it, and then remove the rivet.
| REASSEMBLY SERVICE POINT
| >>A<< RIVETS B / RIVETS A INSTALLATION
| Use recommended tool shown in the illustration to connect the rivet by the following procedure. Insert rivets A and rivets B into the front bumper face and front bumper upper plate. Place the recommended tool over section C of rivet. While pushing the flange surface of the rivet with the recommended tool, press the handle of the tool. The thin part of section C of the rivet will break and the rivet will then be attached.

[51] EXTERIOR - - FRONT BUMPER ASSEMBLY - FRONT BUMPER ASSEMBLY - DISASSEMBLY AND REASSEMBLY <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation