[26] FRONT AXLE - - SPECIFICATION(S) - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SPECIFICATION(S)

SERVICE SPECIFICATIONS
Item | Standard value | Limit
--- | --- | ---
Wheel bearing axial play mm | - | 0.05
Hub starting torque N·m | - | 1.8
Protruding length of stabilizer link mm | <2000-Non-Turbo> | 22 ± 1.5 | -
<2000-Turbo, 2400> | 9.4 ± 0.4 | -
Setting of PTJ boot length mm | <2000> | 90 ± 3 | -
<2400> | 85 ± 3 | -
Opening dimension of the special tool (MB991561) mm | When the BJ boot band (small) is crimped | 2.9 | -
When the BJ boot band (large) is crimped | 2.9 | -
Crimped width of the BJ boot band mm | 2.4 - 2.8 | -

[26] FRONT AXLE - - SPECIFICATION(S) - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation