[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - A/T CONTROL COMPONENT CHECK - STEERING SHIFT SWITCH CHECK <5A/T> | PRINT PAGE / INDEX / PRIOR / NEXT

| STEERING SHIFT SWITCH CHECK <5A/T> Remove the steering wheel lower cover.
| Disconnect the steering shift switch connector and measure the resistance between terminals 1 and 2. Standard value:
Steering shift switch | Resistance value (Ω)
--- | ---
Upshift and hold | 990 - 1, 010
Downshift and hold | 388 - 396
In other than above, replace the driver's air bag module. (Refer to GROUP 52B - Air bag module and clock spring .)

[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - A/T CONTROL COMPONENT CHECK - STEERING SHIFT SWITCH CHECK <5A/T> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation