[25] PROPELLER SHAFT - - SPECIFICATION(S) - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SPECIFICATION(S)

SERVICE SPECIFICATIONS
Item | Standard value | Limit
--- | --- | ---
Propeller shaft run-out mm | - | 0.6
Clearance between snap ring and snap ring groove mm | 0.02 - 0.06 | -

[25] PROPELLER SHAFT - - SPECIFICATION(S) - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation