[42] BODY - - DOOR - DOOR GLASS AND REGULATOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

DOOR GLASS AND REGULATOR

REMOVAL AND INSTALLATION
Pre-removal Operation Door Trim Assembly Removal (Refer to GROUP 52A, Door Trim .) Waterproof Film Removal (Refer to .) | Post-installation Operation Door Window Glass Adjustment (Refer to .) Waterproof Film Installation (Refer to .) Door Trim Assembly Installation (Refer to GROUP 52A, Door Trim .)
|  | Power window switch removal steps
--- | --- | ---
| >>B<< | • | Post-installation operation check <Vehicles for Argentina>
|  | 1. | Power window switch (Refer to GROUP 52A, Door trim .)
|  | Door window regulator assembly removal steps
| >>B<< | • | Post-installation operation check <Vehicles for Argentina>
<<A>> | >>A<< | 2. | Window regulator assembly
<<A>> |  | 3. | Power window motor assembly
|  | Door window glass removal steps
|  | • | Window glass runchannel <Rear door> (Refer to .)
|  | • | Lower sash <rear door> (Refer to .)
|  | • | Door latch assembly <Rear door> (Refer to .)
|  | • | Door beltline molding (Refer to .)
|  | • | Door beltline inner weatherstrip (Refer to .)
|  | 4. | Door window glass
| REMOVAL SERVICE POINT
| <<A>> WINDOW REGULATOR ASSEMBLY/POWER WINDOW MOTOR ASSEMBLY REMOVAL Remove the door window glass installation bolts. CAUTION If tinting film is adhered to the door window glass, attach special tool window glass holder (MB990480) to the outside of the glass to prevent the film from peeling off.
| Lift the door window glass, and attach special tool window glass holder (MB990480) to the glass as shown to prevent the glass from falling. Remove the window regulator assembly and power window motor assembly.
| INSTALLATION SERVICE POINTS
| >>A<< WINDOW REGULATOR ASSEMBLY INSTALLATION
| When installing the window regulator assembly, tighten the bolts to the specified torque in the order shown.
| >>B<< Post-installation operation check <Vehicles for Argentina> When the following procedures are carried out, make the power window switch learn the fully closed position of the power window. (Refer to .) Power window regulator removal or replacement Power window switch removal or replacement

[42] BODY - - DOOR - DOOR GLASS AND REGULATOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation