[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - POWER WINDOWS - INSPECTION PROCEDURE D-6: The window glass lowers automatically while it is rising. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE D-6: The window glass lowers automatically while it is rising.
| COMMENTS ON TROUBLE SYMPTOM If the sliding resistance is too great when the window is being raised or the window glass encounters an object, the window glass will lower by approximately 150 mm.
| POSSIBLE CAUSES Improper adjusted door window glass Incorrectly installed or warped glass slider Malfunction of the power window motor Malfunction of the window regulator
| DIAGNOSIS PROCEDURE
| Step 1. Check the power window anti-trap function. <vehicles for Argentina> Check that the power window anti-trap function works. Refer to GROUP 42 - Door - On-vehicle Service . Q: Is the check result normal? YES: Go to Step 2. NO: Refer to Inspection Procedure D-7 "Power window anti-trap function does not work normally <vehicles for Argentina>."
| Step 2. Check the power window operating current. Check that the power window operating current is normal (Refer to GROUP 42 - Door - On-vehicle service ). Q: Is the check result normal? YES: Adjust the door window glass (Refer to GROUP 42 - Door - On-vehicle service ), and then go to Step 3. NO: Replace the defective power window motor assembly which operating current are abnormal.
| Step 3. Check that the door window glasses are installed correctly. Check that the door window glasses are installed correctly. Refer to GROUP 42 - Door - On-vehicle Service . Q: Is the check result normal? YES: Go to Step 4. NO: Adjust the door window glass (Refer to GROUP 42 - Door - On-vehicle service ).
| Step 4. Retest the system. Check that the power window does not lower automatically while it is being raised. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the power window motor assembly of the defective window.

[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - POWER WINDOWS - INSPECTION PROCEDURE D-6: The window glass lowers automatically while it is rising. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation