[27] REAR AXLE - - REAR AXLE <4WD> | PRINT PAGE / INDEX / PRIOR / NEXT

REAR AXLE <4WD>
The rear axle has the following features: The wheel bearing is a double-row angular contact ball bearing which incorporates the oil seals and is highly resistant to a thrust load. The drive shaft has BJ-TJ constant velocity joints. A smaller BJ side boot is used. ABS rotor for detecting the wheel speed is press-fitted to the BJ outer wheel. <Vehicles with ABS> NOTE: BJ: Birfield Joint TJ: Tripod Joint
SPECIFICATIONS
Item | Specification
--- | ---
Wheel bearing | Type | Double-row angular contact ball bearing
Bearing (OD x ID) mm | 70 × 40
Drive shaft | Type | Outer | BJ
Inner | TJ
Length (joint to joint) × outer diameter mm | LH <2400> | 481 × 22
LH <2000-Turbo> | 468 × 22.2
RH <2400> | 571 × 22
RH <2000-Turbo> | 558 × 22.2
CONSTRUCTION DIAGRAM

[27] REAR AXLE - - REAR AXLE <4WD> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation