[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - POWER WINDOWS - INSPECTION PROCEDURE D-2: Driver's power window does not work by means of the power window main switch. <except vehicles for Argentina> | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE D-2: Driver's power window does not work by means of the power window main switch. <except vehicles for Argentina>
| COMMENTS ON TROUBLE SYMPTOM If the driver's power window does not work by means of the power window main switch, the power window main switch or the driver's door power window motor may be defective.
| POSSIBLE CAUSES Malfunction of the power window main switch Malfunction of the power window motor (front RH) <R.H. drive vehicles> Malfunction of the power window motor (front LH) <L.H. drive vehicles> Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Check the power window main switch. Check that all of the front passenger's and rear door power windows can operate by means of the power window main switch. Q: Is the check result normal? YES: Go to Step 2. NO: Refer to Inspection Procedure D-1 "Power windows do not work at all <except vehicles for Argentina>."
| Step 2. Connector check: E-05 power window main switch connector Q: Is the check result normal? YES: Go to Step 3. NO: Repair the connector.
| Step 3. Check the power window main switch. Refer to GROUP 42 - Door . Q: Is the check result normal? YES <R.H. drive vehicles>: Go to Step 4. YES <L.H. drive vehicles>: Go to Step 10. NO: Replace the power window main switch.
| Step 4. Measure the voltage at the E-05 power window main switch connector. Disconnect the connector, and measure at the wiring harness side. Turn the ignition switch to the ON position. Voltage between terminal 13 and body earth OK: Battery positive voltage Q: Is the check result normal? YES: Go to Step 7. NO: Go to Step 5.
| Step 5. Connector check: C-208 power window relay connector Q: Is the check result normal? YES: Go to Step 6. NO: Repair the connector.
| Step 6. Check the wiring harness between C-208 power window relay connector terminal No.4 and E-05 power window main switch connector terminal No.13. NOTE: Prior to the wiring harness inspection, check intermediate connectors C-15, E-29 and junction block connector C-203, and repair if necessary. Check the power supply line for open circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00, How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 7. Connector check: E-23 power window motor (front RH) connector Q: Is the check result normal? YES: Go to Step 8. NO: Repair the connector.
| Step 8. Check the power window motor (front RH). Refer to GROUP 42 - Door . Q: Is the check result normal? YES: Go to Step 9. NO: Replace the power window motor (front RH).
| Step 9. Check the wiring harness from E-23 power window motor (front RH) connector terminal Nos.1 and 4 to E-05 power window main switch connector terminal Nos.8 and 9. NOTE: Prior to the wiring harness inspection, check intermediate connector E-29, and repair if necessary. Check the power window operating lines for open or short circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00, How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 10. Measure the voltage at the E-05 power window main switch connector. Disconnect the connector, and measure at the wiring harness side. Turn the ignition switch to the ON position. Voltage between terminal 13 and body earth OK: Battery positive voltage Q: Is the check result normal? YES: Go to Step 13. NO: Go to Step 11.
| Step 11. Connector check: C-208 power window relay connector Q: Is the check result normal? YES: Go to Step 12. NO: Repair the connector.
| Step 12. Check the wiring harness between C-208 power window relay connector terminal No.4 and E-05 power window main switch connector terminal No.13. NOTE: Prior to the wiring harness inspection, check intermediate connectors C-118, E-12 and junction block connector C-203, and repair if necessary. Check the power supply line for open circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00, How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 13. Connector check: E-13 power window motor (front LH) connector Q: Is the check result normal? YES: Go to Step 14. NO: Repair the connector.
| Step 14. Check the power window motor (front LH). Refer to GROUP 42 - Door . Q: Is the check result normal? YES: Go to Step 15. NO: Replace the power window motor (front LH).
| Step 15. Check the wiring harness from E-13 power window motor (front LH) connector terminal Nos.1 and 4 to E-05 power window main switch connector terminal Nos.8 and 9. NOTE: Prior to the wiring harness inspection, check intermediate connector E-12, and repair if necessary. Check the power window operating lines for open or short circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00, How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.

[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - POWER WINDOWS - INSPECTION PROCEDURE D-2: Driver's power window does not work by means of the power window main switch. <except vehicles for Argentina> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation