[13B] MULTIPORT FUEL INJECTION (MPI) <4G64> - - ON-VEHICLE SERVICE - COMPONENT LOCATION | PRINT PAGE / INDEX / PRIOR / NEXT

COMPONENT LOCATION
Name | Symbol | Name | Symbol
--- | --- | --- | ---
Air flow sensor (with intake air temperature sensor and barometric pressure sensor) | G | Engine-A/T-ECU | S
A/C relay | N | Engine warming lamp (check engine lamp) | P
A/C switch | R | Fan controller | M
A/C pressure sensor | A | Fuel pump relay (1) and (2) | O
Camshaft position sensor | K | Idle speed control servo | F
Crank angle sensor | I | Ignition coil | J
Detonation sensor | B | Injectors | D
Diagnosis connector | Q | Inhibitor switch | N
EGR control solenoid valve | C | Mixture adjusting screw <Vehicles without catalytic converter> | G
Engine coolant temperature sensor | K | Power steering fluid pressure switch | H
Engine control relay | N | Throttle position sensor | E

[13B] MULTIPORT FUEL INJECTION (MPI) <4G64> - - ON-VEHICLE SERVICE - COMPONENT LOCATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation