[11D] ENGINE OVERHAUL <4G6-DOHC> - - GENERAL SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL SPECIFICATIONS
Item | Specification
--- | ---
Bore × stroke mm | 85 × 88
Displacement mL | 1,997
Combustion chamber | Pentroof type
Number of cylinders | 4
Valve mechanism | Type | Double overhead camshaft
Number of intake valves | 2
Number of exhaust valves | 2
Lash adjusters | Hydraulic
Rocker arms | Roller cam followers
Compresssion ratio | 9.0
Fuel injection system | Electronically controlled multi-point injection (MPI) system
Ignition system | Electronically controlled two-coil system
Generator | Alternator (with built-in IC regulator)
Starter motor | Gear reduction drive type

[11D] ENGINE OVERHAUL <4G6-DOHC> - - GENERAL SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation