[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - ON-VEHICLE SERVICE - INTAKE AIR TEMPERATURE SENSOR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| INTAKE AIR TEMPERATURE SENSOR CHECK
| Disconnect the air flow sensor connector. Measure resistance between terminals No. 5 and No. 6. Standard value: 13 - 17 kΩ (at -20°C) 5.3 - 6.7 kΩ (at 0°C) 2.3 - 3.0 kΩ (at 20°C) 1.0 - 1.5 kΩ (at 40°C) 0.56 - 0.76 kΩ (at 60°C) 0.30 - 0.42 kΩ (at 80°C) Remove the air flow sensor
| Measure resistance while heating the sensor using a hair drier.
Normal condition:
Temperature (°C) | Resistance (kΩ)
--- | ---
Higher | Smaller
| If the value deviates from the standard value or the resistance remains unchanged, replace the air flow sensor assembly. Install the air flow sensor and tighten it to the specified torque. Tightening torque: 8.8 ± 1 N·m

[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - ON-VEHICLE SERVICE - INTAKE AIR TEMPERATURE SENSOR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation