[54A] CHASSIS ELECTRICAL - - SIDE TURN-SIGNAL LAMP - SIDE TURN-SIGNAL LAMP - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

SIDE TURN-SIGNAL LAMP

REMOVAL AND INSTALLATION
|  |  | Removal steps
--- | --- | --- | ---
<<A>> | >>A<< | 1. | Side turn-signal lamp assembly
|  | 2. | Side turn-signal lamp
|  | 3. | Bulb
|  | 4. | Socket
| REMOVAL SERVICE POINT
| <<A>> SIDE TURN-SIGNAL LAMP REMOVAL
| Use a special tool ornament remover (MB990784), etc. to remove the side turn-signal lamp by pushing the fender forward, bending the hook, and then unclamping the thumb.
| INSTALLATION SERVICE POINT
| >>A<< SIDE TURN-SIGNAL LMP INSTALLATION
| Clamp the thumb on the fender panel the assemble the side turn-signal lamp.

[54A] CHASSIS ELECTRICAL - - SIDE TURN-SIGNAL LAMP - SIDE TURN-SIGNAL LAMP - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation