[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - CATALYTIC CONVERTER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

CATALYTIC CONVERTER

REMOVAL AND INSTALLATION
|  |  | Removal steps
--- | --- | --- | ---
<<A>> | >>A<< | 1. | Oxygen sensor <4G63, 4G69 (Vehicles for Brazil, Chile)>
|  | 2. | Centre exhaust pipe connection
|  | 3. | Exhaust pipe gasket
|  | 4. | Front exhaust pipe connection
|  | 5. | Exhaust pipe gasket
|  | 6. | Catalytic converter
| REMOVAL SERVICE POINT
| <<A>> OXYGEN SENSOR REMOVAL
| Use special tool oxygen sensor wrench (MD998770) to remove the oxygen sensor.
| INSTALLATION SERVICE POINT
| >>A<< OXYGEN SENSOR INSTALLATION
| Use special tool oxygen sensor wrench (MD998770) to install the oxygen sensor.

[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - CATALYTIC CONVERTER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation