[55A] HEATER, AIR CONDITIONER AND VENTILATION - - REFRIGERANT LINE - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

REFRIGERANT LINE

REMOVAL AND INSTALLATION
Pre-removal and Post-installation Operation Refrigerant Draining and Refilling (Refer to Charging and Discharging ). Air cleaner cover and air flow sensor assembly Removal and Installation (Refer to GROUP 15, Air cleaner <2400-except MIVEC>, <2400-MIVEC>). Radiator Grille Removal and Installation (Refer to GROUP 51, Radiator Grille <2000>, <2400>).
|  |  | Removal steps
--- | --- | --- | ---
<<A>> |  | 1. | A/C pressure sensor
<<A>> |  | 2. | Flexible discharge hose
<<A>> | >>A<< | 3. | Flexible suction hose
<<A>> |  | 4. | Liquid pipe B
|  | 5. | Evaporator cover
<<A>> |  | 6. | Liquid pipe A
|  | 7. | O ring
| REMOVAL SERVICE POINT
| <<A>> HOSE/PIPE DISCONNECTION CAUTION As the compressor oil and receiver are highly moisture absorbent, use a non-porous material to plug the hose and nipples. To prevent the entry of other foreign bodies, plug the condenser, compressor, and expansion valve nipples.
| INSTALLATION SERVICE POINT
| >>A<< SUCTION HOSE INSTALLATION When replacing the suction hose, refill them with a specified amount of compressor oil, and then install them. Compressor oil: SUN PAG 56 Quantity: Suction hose: 10 cm3

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - REFRIGERANT LINE - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation