[51] EXTERIOR - - GARNISHES - GARNISHES - REMOVAL AND INSTALLATION <20V, R, GLX, LS> | PRINT PAGE / INDEX / PRIOR / NEXT

GARNISHES

REMOVAL AND INSTALLATION <20V, R, GLX, LS>
|  |  | Removal steps
--- | --- | --- | ---
|  | • | Front deck garnish (Refer to ).
<<A>> | >>A<< | 1. | Side sill garnish
DOUBLE-SIDED TAPE AFFIXED LOCATION
| REMOVAL SERVICE POINT
| <<A>> SIDE SILL GARNISH REMOVAL Gently lift and remove the side sill garnish. If there is any double-sided tape remaining on the side sill garnish, remove according to the following instructions. <Remove double-sided tape remaining on the body surface>
| Attach protection tape all the way along the edges of the double-sided tape which is still adhering to the body.
| Scrape off the double-sided tape with a resin spatula as possible. Peel off the protection tape. Wipe the body surface and clean it with a rag moistened with isopropyl alcohol.
| <Remove double-sided tape remaining on side sill garnish and adhere double-sided tape (when re-using side sill garnish)>
| Scrape off the double-sided tape on the side sill garnish with a resin spatula as possible. Wipe the side sill garnish surface and clean it with a rag moistened with isopropyl alcohol. Remove only a small portion of the residual adhesive. Adhere the double-sided tape as specified on the side sill garnish. (Refer to double-sided tape adherence location .)
| INSTALLATION SERVICE POINT
| >>A<< SIDE SILL GARNISH INSTALLATION
| Tear off the double-sided tape backing paper. NOTE: If you attach the adhesive tape to the edge of the backing paper, it will be easy to tear off. Install the side sill garnish. NOTE: If the double-sided tape is difficult to affix in cold temperature, etc., warm the bonding surfaces of the body and side sill garnish to about 40 - 60°C before affixing the tape. Firmly press in the side sill garnish.

[51] EXTERIOR - - GARNISHES - GARNISHES - REMOVAL AND INSTALLATION <20V, R, GLX, LS> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation